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PROCUREMENT SPECIFICATIONS FOR TRANSISTORS
AS PER MIL SPECIFICATIONS

DETAILS

Package

PartNumber | Detail Specification
2N3637 i MIL-PRE-19500/357

B. DEVICE QUALITY

1. Devices shall be Qualified to JANS of MIL-PRE-19500.

2. All parts shall undergo Manufacturer’s Pre-cap Visual Inspection as part of MIL-PRF-
19500,

3. All parts shall be serialized and screened as per MIL-PRF-19500.

4. Three samples drawn from the deliverable quantity shall undergo Destructive Physical
Analysis (DPA).

C. DATAPACK REQUIREMENTS

The following Data shall accompany the devices in soft copy (compact disk)
1. Read and Record data of
a. Delta parameters — Pre and Post HTRB (if applicable), Pre and Post Burn-in with
deltas calculated.
b. Report of 100% final electrical parameters measurements as per Group A,
subgroups 2 and 3.
. Group A, Group B and Group C test reports as applicable.
DPA test report,
Manufacturer's Pre-cap Visual Inspection report.
. Certificate of Conformance issued by the Manufacturer.

D. OTHER REQUIREMENTS

The name of the manufacturer shall be specified as part of the offer.

2. Devices shall be supplied preferably from lois with same date code. The devices shall
be drawn from lots manufactured preferably within 2 years of the date of shipment
Devices shall be individually packed.

4. Only Vendors/suppliers authorized to source above Space Grade components from the
Manufacturer will be considered. Necessary Certificate from the Manufacturer shall be
enclosed along with the offer.
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E. RESPONSIBILITIES OF THE SUPPLIER

The supplier shall undertake following additional tasks to ensure that the devices meet the

necessary quality requirements:

1. Monitor manufacturers where required and perform Final Customer Source Inspection
(FCSI).

2. Perform 100% Incoming Inspection and Data pack review before shipment.

3. Report to ISAC all NCR/DCN during procurement/ testing.

Please provide the point-by-point compliance to specification in your quote.
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